uint64 timestamp	# time since system start (microseconds)
uint64 timestamp_utc # UTC timestamp

uint32 seq		# Image sequence number
bool feedback	# Trigger feedback from camera

uint32 ORB_QUEUE_LENGTH = 2
