uint64 timestamp		# time since system start (microseconds)

uint8 active_sys_id		# mavlink system id of the currently active camera
uint8 active_comp_id 	# mavlink component id of currently active camera
