## Used to command an actuation in the gripper, which is mapped to a specific output in the control allocation module

uint64 timestamp

int8 command		# Commanded state for the gripper
int8 COMMAND_GRAB = 0
int8 COMMAND_RELEASE = 1
